Base station:

Esp32-wroom-32u:

-Connection to motor

-connection with encoder

-running server, and response to incoming requests:

- feedback data

- operate from remote

Example for motor connection

([Basics\_%20Project%20072u%20ESP32%20Development%20board%20with%20DC%20Motor%20and%20L298N%20H-Bridge%20motor%20driver%20module%20at%20Acoptex.com%20\_%20ACOPTEX.COM.html](file:///C:/_RAN_FILES_/SourceTree/Alin/code/32u%20board/Basics_%20Project%20072u%20ESP32%20Development%20board%20with%20DC%20Motor%20and%20L298N%20H-Bridge%20motor%20driver%20module%20at%20Acoptex.com%20_%20ACOPTEX.COM.html) )

